【Mass Production】
Lithium fluorosulfonate EMC solution
氟磺酸锂碳酸甲乙酯溶液

▎ Basic Information
	Abbreviation
	LiSO3F-EMC

	[bookmark: _GoBack]Product Status
	Mass Production


▎ Technical Specifications
	Test Item
	Specification

	Purity
	≥99.0 %

	Moisture
	≤100 ppm

	Free Acid
	≤2000 ppm

	Chloride (Cl⁻)
	≤20 ppm

	Sulfate (SO₄²⁻)
	≤2000 ppm



Note: The above technical specifications are typical values. Specific specifications are subject to the Certificate of Analysis (COA). For detailed product information or customized specifications, please contact our sales team.
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